**SUNRISE EVALUATION EXAMS F4**

***Kenya Certificate of Secondary Education***

**441/2**

**CLOTHING AND TEXTILES**

**PAPER 2**

**PRACTICAL**

**TIME: 2½ HOURS**

**MARKING SCHEME**

**STUDENT’S NAME …………………………….…………………INDEX NO. ………………………..…**

|  |  |  |  |
| --- | --- | --- | --- |
| **1. PRESENTATION** | **MAX SCORE** | **SCORE** | **REMARKS** |
| * 1. Folding the article neatly   2. Firmly sewn on label on single fabric   3. Pins, needles and unnecessary tacking removed from work   4. Clean and press | 1  1  1  1 |  |  |
|  | **4** |  |  |
| **2. CUTTING OUT**   1. Centre front and centre back straight 2. Good cutting and grain line on: 3. Skirt front 4. Skirt back 5. Pocket 6. Front yoke 7. Identification of right half of skirt | 1  ½  ½  ½  ½  1 |  |  |
|  | **4** |  |  |
| **3. BACK DART**   1. Accuracy in length (½) width(½) 2. Stitchery tapering to a point (½) 3. Correct tension (½ ) size (½) straight (½ ) 4. Flat on both sides R.S. (½) W.S (½) 5. Dart secured at the point (1) 6. Pressed towards the centre front (1) | 1  ½  1½  1  1  1 |  |  |
|  | **6** |  |  |
| **4. PREPARATION OF GATHERS**   1. Correct position (½) (lower front piece) 2. Well distributed(½) 3. Well held in position (½) 4. Correct stitches (Gathering stitches) (½) | ½  ½  ½  ½ |  |  |
|  | **2** |  |  |
| **5. ATTACHING THE YOKE**   1. Flat (½) 2. Folded edge of yoke (½) placed on F.L of front skirt (½) 3. Stitchery 2mm away from fold (½) 4. Even distribution of gathers (½) 5. Stitchery – straight (½) correct tension (½) size (½) 6. Trimming of seam turning to “¼” (½) 7. Neatening of seam allowance using loop stitches (1) correct tension of loop stitches (½) | ½  ½  ½  ½  1½  ½  1½ |  |  |
|  | **6** |  |  |
| **6. ATTACHING POCKET INSEAM**   * 1. Accurate use of F.L when attaching pocket pieces to skirt front (½) back (½)   2. Correct position (1)   3. Correct shape (1) and size (1)   4. Reinforcing of pocket mouth (1)   5. Correct width of mouth ½ inches (1) | 1  1  2  1  1 |  |  |
|  | **6** |  |  |
| **7. SIDE SEAM (UNNEATENED)**   * 1. Accurate use of the F.L (1)   2. Pressing seam open (1)   3. Untrimmed (1) and unneatened (1) above and below the pocket mouth | 1  1  2 |  |  |
|  | **4** |  |  |
| **8. JOINING OF POCKET BAG**   * 1. Joining fitting lines together (1)   2. Pocket facing down wards (1)   3. Firmly joined using open seam (½) edgestrimmed (½) | 1  1  1 |  |  |
|  | **3** |  |  |
| **9. HEMMING SKIRT BACK (SLIP HEMMING)**   * 1. Flat (1)   2. Stitchery  1. Even stitches (½) 2. Slip hemming (½) correct size (1) correct position (1) 3. Slip hemming back skirt (½) half of the hem (½ ) 4. Correct finished width 1 inch (1) | 1  ½  2 ½  1  1 |  |  |
|  | **6** |  |  |