**SUNRISE EVALUATION EXAMS F4**

***Kenya Certificate of Secondary Education***

**441/2**

**CLOTHING AND TEXTILES**

**PAPER 2**

**PRACTICAL**

**TIME: 2½ HOURS**

**MARKING SCHEME**

**STUDENT’S NAME …………………………….…………………INDEX NO. ………………………..…**

|  |  |  |  |
| --- | --- | --- | --- |
| **1. PRESENTATION**  | **MAX SCORE**  | **SCORE** | **REMARKS** |
| * 1. Folding the article neatly
	2. Firmly sewn on label on single fabric
	3. Pins, needles and unnecessary tacking removed from work
	4. Clean and press
 | 1111 |  |  |
|  | **4** |  |  |
| **2. CUTTING OUT**1. Centre front and centre back straight
2. Good cutting and grain line on:
3. Skirt front
4. Skirt back
5. Pocket
6. Front yoke
7. Identification of right half of skirt
 | 1½½½½1 |  |  |
|  | **4** |  |  |
| **3. BACK DART** 1. Accuracy in length (½) width(½)
2. Stitchery tapering to a point (½)
3. Correct tension (½ ) size (½) straight (½ )
4. Flat on both sides R.S. (½) W.S (½)
5. Dart secured at the point (1)
6. Pressed towards the centre front (1)
 | 1½1½111 |  |  |
|  | **6** |  |  |
| **4. PREPARATION OF GATHERS**1. Correct position (½) (lower front piece)
2. Well distributed(½)
3. Well held in position (½)
4. Correct stitches (Gathering stitches) (½)
 | ½½½½ |  |  |
|  | **2** |  |  |
| **5. ATTACHING THE YOKE** 1. Flat (½)
2. Folded edge of yoke (½) placed on F.L of front skirt (½)
3. Stitchery 2mm away from fold (½)
4. Even distribution of gathers (½)
5. Stitchery – straight (½) correct tension (½) size (½)
6. Trimming of seam turning to “¼” (½)
7. Neatening of seam allowance using loop stitches (1) correct tension of loop stitches (½)
 | ½½½½1½  ½ 1½ |  |  |
|  | **6**  |  |  |
| **6. ATTACHING POCKET INSEAM*** 1. Accurate use of F.L when attaching pocket pieces to skirt front (½) back (½)
	2. Correct position (1)
	3. Correct shape (1) and size (1)
	4. Reinforcing of pocket mouth (1)
	5. Correct width of mouth ½ inches (1)
 | 11211 |  |  |
|  | **6** |  |  |
| **7. SIDE SEAM (UNNEATENED)*** 1. Accurate use of the F.L (1)
	2. Pressing seam open (1)
	3. Untrimmed (1) and unneatened (1) above and below the pocket mouth
 | 112 |  |  |
|  | **4** |  |  |
| **8. JOINING OF POCKET BAG** * 1. Joining fitting lines together (1)
	2. Pocket facing down wards (1)
	3. Firmly joined using open seam (½) edgestrimmed (½)
 | 111 |  |  |
|  | **3** |  |  |
| **9. HEMMING SKIRT BACK (SLIP HEMMING)*** 1. Flat (1)
	2. Stitchery
1. Even stitches (½)
2. Slip hemming (½) correct size (1) correct position (1)
3. Slip hemming back skirt (½) half of the hem (½ )
4. Correct finished width 1 inch (1)
 | 1½2 ½11 |  |  |
|  | **6** |  |  |